Navitia data injection steps : To poor GTFS on the dedicated Navitia instance :

* http to the VM URL/v1/coverage/default/lines
* Open the sat-up SFTP client and connect to the VM
* Get to /srv/ed/input/default
* Drop the GTFS/PBF file
* When the dropped file disappears
* Wait for a couple of minutes for the file to be ingested by Navitia
* Refresh the HTTP to the VM URL/v1/coverage/default/lines to confirm the GTFS ingestion